**Tender CUI/ATD/32/Biotech (2020-2021)**

|  |  |  |
| --- | --- | --- |
| **Tender S#** | **Description** | **Quantity Required** |
| 1 | Trans Illuminator  Light Source: 4 x 8 Watt UV bulbs  Wavelength: 302nm  Intensity Control: Low (50%) or High (100%)  Viewing Surface: 16 x 19cm  Electrical: 220V, 50-60Hz  Warranty: 2 Years | 01 No |
| 2 | Laminar Flow Hood  Customized:  Structure: Vertical  Material: Stainless Steel  Application: Lab  Type: Clean Bench  Cleaning Level: Grade 100 (209e U.S. Federal)  Several Colonies: ≤0.5per Utensil. Hour (90mm Utensil)  The Average Wind Speed: 0.25 ~0.454m/S (Speed Two – Speed)  Noise: ≤62dB  Power: AC, Single 220 V/50Hz  Illumination: ≥300lx  Max. Power Consumption: 300W  Weight: <85kg  Dimension of working: 700\*500\*520mm | 01 No |
| 3 | Camera  Photography: Full HD Movie: Yes, Rear Camera Pixel: 18.0  Features: LCD Size: 3.0 Inch, Build in Flash: Yes, Memory Type: SD  Warranty: 1 Year genuine  Hardware: Battery Life: 440 Shoots | 01 No |