**Tender CUI/ATD/32/Biotech (2020-2021)**

|  |  |  |
| --- | --- | --- |
| **Tender S#** | **Description** | **Quantity Required** |
| 1 | Trans IlluminatorLight Source: 4 x 8 Watt UV bulbsWavelength: 302nmIntensity Control: Low (50%) or High (100%)Viewing Surface: 16 x 19cmElectrical: 220V, 50-60HzWarranty: 2 Years | 01 No |
| 2 | Laminar Flow HoodCustomized: Structure: VerticalMaterial: Stainless SteelApplication: LabType: Clean BenchCleaning Level: Grade 100 (209e U.S. Federal)Several Colonies: ≤0.5per Utensil. Hour (90mm Utensil)The Average Wind Speed: 0.25 ~0.454m/S (Speed Two – Speed)Noise: ≤62dBPower: AC, Single 220 V/50HzIllumination: ≥300lxMax. Power Consumption: 300WWeight: <85kgDimension of working: 700\*500\*520mm | 01 No |
| 3 | CameraPhotography: Full HD Movie: Yes, Rear Camera Pixel: 18.0Features: LCD Size: 3.0 Inch, Build in Flash: Yes, Memory Type: SDWarranty: 1 Year genuineHardware: Battery Life: 440 Shoots | 01 No |